
	Terminal Server Manager (TSM) V2.1-09 
	Web Distribution Kit TSM_README.TXT

	This is a remastered kit containing TSM V2.1-09. It contains all
	of the fixes included in TSM V2.1 ECOs 1 through 9, as well as
	a modern set of documentation available in PDF format, as Post-
	script files have become an anachronism in the 25 years since
	ECO 9 was released.

	The updating of this kit and documentation was performed by
	Teresa Kennedy <terry-decus@glaver.org> and should not be con-
	sidered an official DEC / Compaq / HP distribution. However, it
	was built from the last TSM sources before TSM was discontinued.

	The files in this directory are as follows:

		TSM021_DCX_VAX.EXE
		TSM021_DCX_AXP.EXE
		TSM_PAK.COM
		TSM_README.TXT

	The TSM_PAK.COM file will register and load a License Management
	Facility (LMF) Product Authorzation Key (PAK) for TSM. You may or
	may not need to execute this VMS command file, depending on the 
	availability of a TSM license in LMF.

		$ @TSM_PAK.COM

	The TSM021_DCX_VAX.EXE file is an OpenVMS / VAX executable file.
	To extract the contents on a VAX system, run it .  

		$ RUN TSM021_DCX_VAX.EXE	

	The TSM021_DCX_AXP.EXE file is an OpenVMS / AXP executable file.
	To extract the contents on a Alpha system, run it .  

		$ RUN TSM021_DCX_AXP.EXE

	You will get a resultant file (name dependent on what you told 
	the decompression utility to use for an output file name), which
	is an Open VMS SAVESET.

		e.g. TSM021.SAV

	Create a working directory, for example:

		$ CREA /DIR [.TSM]

	Don't do this in an area (default directory) that is a VMS 
	LOGICAL that uses those funky VMS search lists.  Examples of 
	this are:

		SYS$MANAGER: and SYS$UPDATE:
	
	
	Extract the saveset into the working directory:

		$ BACKUP TSM021.SAV /SAVE [.TSM...]

	Then execute the OpenVMS installation procedure in the normal 
	fashion:

		$ @SYS$UPDATE:VMSINSTAL

	The location of the kit directory should be the fully specified
	path to the [.KIT] subdirectory in the working directory you
	created (e.g. DKA100:[JOE.TSM.KIT]).  Don't specify the path
	using system logicals for the disk; use the disk device name.

	The softcopy manuals are to be found in the [.DOCUMENTATION]
	subdirectory of the working directory that you created
	(e.g. DKA100:[JOE.TSM.DOCUMENTATION]).

	Enjoy!



